T. Oest P RC Open Session 8 /7/98 1

Vertex Detector

Installation Status:

final infrastructure 12 double sided detector modules installed (+ 5 in August) final readout chain

movable RF shield (5 μm steel bands) vertex vessel vacuum wo rse than 1997, under investigation

August Shu tdown:

5 mo re mo dules installation of laser system

T. Oest P RC Open Session 8 /7/98 2

Helix Readout Chip

Vertex Detector

Helix 128S- 2.1 (used in 1998) reduced radiation hardness digital- analog cross talk

Helix 128S- 2.2 (since April 1998) new pipeline design tested up to 400 kRad readout at 40 MHz acceptable cross talk close to final readout chip

Helix 128S- 2.3 (under test)

Helix 128S-3. 0 (in progress)

Version 2.2 fulfills HERA- B requirements

Puls shape / dose