50R4

470R29

1pmfC16

10pmfC5150R1150R13

10pmfC52

10pmf10pmfC5350R14-IN15

-IN16

-IN3

-IN4

-IN2
mfC20mfC17mfC39mfC22mfC23mfC38mfC18

-IN6
mfC264,7

R2222kR174,7R204,7

R18

1pmfC450R34,7

R21

50R51pmfC51pmfC3

10uH

mhL1
mfC58mfC60mfC56mfC570/47

47100+IN10

mfC28

1pmfC650R6-IN7

+IN7

-IN8

471pmfC8+IN8

10pmfC4850R950R15-IN1

10pmfC54

10pmfC4947R3050R250R847-IN13

+IN6
mfC19

100n

mfC3650R16

10k

50R10-IN5

-IN9

1pmfC21pmfC750R7

BAT63

50R1

mf

10pmfC55

mfC5962R281pmfC1

NC1GNDD

GNDA4

GNDA3

GNDA2

GNDA1

SUBD

SUBA2

SUBA1

VE3VE2D

VC2D

SB8SA8SB7SA7SB1SA1

OUT5

OUT4

OUT2

OUT1

IN7IN7IN6IN6IN5IN5IN4IN4IN3IN3IN2IN2IN1IN1

IS2ID

TH8TH7

TH4

OUT7

TH6TH5TH3TH2

TH1OUT8

UOT8

OUT6

OUT3

IN8IN8

VE2A

VC2A

VCCIS3

ASD 8 B

I112345678910111213141516171819

20212223242526272829303132

33343536373839404142434445464748495051

5253545556575859606162636410k

4,7R19+IN9

mfC24

BAV99D10-IN14

mfC31mfC33mfC35mfC34mfC30mfC32

-IN10

-IN12

-IN11

50R121pmfC151pmfC141pmfC131pmfC121pmfC111pmfC101pmfC910pmfC47

10KR25

10pmfC46

10pmfC45

10pmfC44

10pmfC43

10pmfC42

10pmfC41

10pmfC4022K

R26
mfC27

+IN5

+IN4

+IN3

+IN2

+IN1

+IN11

+IN12

+IN13

+1IN14

+IN15

+IN16

BAV99D8

BAV99D54,7

R27BAV99D4BAV99D7BAV99D6BAV99D3BAV99D2BAV99D1BAV99D9BAV99D11BAV99D12BAV99D13BAV99D14BAV99D15BAV99D16BAV99D17

I212345678910111213141516171819

52535455565758596061626364

1KR33

DESY-IFH

Zeuthen

Name

TagGepr.

Bearb

the thresh.

for adjusting
install only

ASD8 Preamp.

->pos.

->neg.

100mV=10fC

N3D   24 mA

P3D   40 mA

N3   50 ...65 mA

P3A   47...80 mA

N3A   24 mA

50 ohms

2/96

N3DN3AN3AN3DTHRTPAGND

DGND

161ground- rail

N3N3P3AP3AP3DP3D

HERA_B

M. Pohl

important for stable work

thresh -250mV

=> inp. 1 fC

with CuBe- rails is
between neighbour ampl.

connecting of ground rails
not installed
pinview

positive

10 : 1
testpulse
analog
output

X4X4X3X1