          Target Checklist

Read all notes, please!

 Checked by (name):

 Date/time:

     OK check not-OK action

TaCoS environment is running call expert

tcc is running

no emergencies are displayed in tcc^1

no HV-alarms^2

ZEUS/HERMES display is running

rate distribution display is running

bunchcontribution display is running

ford is running^3

Get an OK from the coordinating experiment call run coordinator

Start Target operation call expert

Set the Autorate to 1MHz

Adjust all emergencies (see note^4)

IA-rate is below 0.25 MHz^5

BG-rate is below 0.25 MHz^6

Select a wire and watch it finding
the beam^7

Rise the Autorate step by step till
you reach desired level^8

1This means: ’target-connection OK’ and ’No Bufferoverflow!’ 2Look at the HV-xterm, if you find any ’malfunction’ or ’alarm’. 3information on Bunchcontribution-display is updated 4Depending on the HERA conditions and your own plans you may alter the values below.

If unsure call expert. Good defaults are:

emergency(OA): 50 MHz
emergency: 30 MHz
emergency(BG): 0.3 MHz
rateloss-detect: 0.010 MHz
rateloss-detect: 10 times

5If you know how, adjust the corresponding parameter in the expert-menu. If unsure call expert! 6Adjust the ’emergency(BG)’ if BG is below 5MHz. If unsure call expert! 7Refer to the short term plan on the run coordination home page.

However II inner is a good choice for single wire runs, which are still default right now. 8Don’t forget to watch the BG’s of the other experiments:

If the BG rate of the other experiments wasn’t red (on the tcc interface) before you inserted the wire, but turns red due to your actions, clearify the situation with the corresponding experiment. If you need assistance please call run coordinator or expert.

     Target -- Run Stop Checklist

Read all notes, please!

 Checked by (name):

 Date/time:

     OK check not-OK action
            Totally move out wires call expert
            Reduce rate to 1MHz
            Deselect each selected wire and wait
            all of them reaching the initial
            position.
            Calibrate all wires
            Comments^{101} mail expert

101Some general comments about the run, any strange or unusual observation.